**EMO, Milan**

**Hall 10, Stand B10**

**940/842 modular grooving system**

This modular grooving system has been developed for smaller machines with shallower groove depths for which 845 cartridges are too large – such as Index machines with W gear teeth for VDI25 or Index machines with dovetail holders.

The 940 modular grooving system for S100 inserts is height-adjustable and provides an integrated coolant supply through its clamping finger and support.

*382 characters incl. spaces*

**Image captions:**



**Image 1:** For smaller machines with shallower groove depths: the 940/842 grooving system.

**Image credits:** Paul Horn GmbH, Nico Sauermann

Text and further information:

Hartmetall-Werkzeugfabrik Paul Horn GmbH, Mr Christian Thiele

Unter dem Holz 33-35, 72072 Tübingen, Germany

Tel.: +49 7071 7004-1602, Fax: +49 7071 72893

E-mail: [christian.thiele@phorn.de](mailto:christian.thiele@phorn.de), [www.phorn.de](http://www.phorn.de/)